Container / Vehicle Packing Certificate

The person responsible for packing the container/vehicle should complete the checklist and sign the certification.

It is declared that that packing of the goods into the unit has been carried out in accordance with the provisions of 5.4.2.1.

It is certified that the packing of the cargo transport unit: has been carried out in accordance with the following conditions:

The cargo transport unit was clean, dry and apparently fit to receive the goods.

If the consignment includes goods of class 1, other than division 1.4, the cargo transport unit is structurally serviceable in conformity with 7.4.6.

Goods which should be segregated have not been packed together onto or in the cargo transport unit (unless approved by the competent authority concerned in accordance with 7.2.2.3).

All packages have been externally inspected for damage, leakage or sifting, and only sound packages loaded.

Drums have been stowed in an upright position, unless otherwise authorized by the competent authority.

All packages have been properly packed onto or in the cargo transport unit and secured.

When dangerous goods are transported in bulk packaging, the cargo has been evenly distributed

The cargo transport unit and the packages therein are properly marked, labeled and placarded.

When solid carbon dioxide (CO2 - dry ice) is used for cooling purposes, the cargo transport unit is externally marked or labeled in a conspicuous place, such as at the door end, with the words: “DANGEROUS CO2 GAS (DRY ICE) INSIDE. VENTILATE THOROUGHLY BEFORE ENTERING”.

The dangerous goods transport document required in 5.4.1 has been received for each dangerous goods consignment packed onto or in the cargo transport unit.

Company / Organization of Signatory

Typed Name / Signature

Date / Location

IFI Form: TC3 Provided by International Forwarders, Inc.

Your Global Logistics Partner

Container / Vehicle Packing Certificate

exp-user

2003-06-23

International Forwarders Inc.